======================================================
Bosch BNO055 9-axis absolute orientation sensor driver
======================================================

This software component contains the Bosch Sensortec MEMS BNO055 sensor driver (sensor API).
Refer to http://www.bosch-sensortec.com/bst/products/all_products/bno055 for more details.

The BNO055 is a system in package (SiP) chip that includes a 3-axis 14-bit
accelerometer, a 3-axis 16-bit gyroscope and a 3-axis magnetometer.

Features
--------

* Initialization the sensor with I2C communication
* Power mode configuration of the sensor
* Reading data from sensor

Dependencies
------------

* An instance of the I2C Master Sync driver is used by this driver.

Limitations
-----------

* IO read/write operation should be synchronous
